<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.3.00.200T">
    <devices>
        <dev id="A51DDDDF-B454-4be8-87C4-FDBEFC28939B" name="PC1" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-07-54-88  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-07-54-88" com_port="0" bootmode="0" cx="305.000000" cy="553.000000" edit_left="332" edit_top="607">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="5BE3F837-9383-4154-8548-82499F00E916" name="PC2" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-C4-01-69  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-C4-01-69" com_port="0" bootmode="0" cx="430.000000" cy="553.000000" edit_left="457" edit_top="607">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="AC4714D7-D1C0-4058-8109-31FAEFDB2A2C" name="PC3" poe="0" model="PC" settings=" -simpc_ip 192.168.3.100  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.3.254  -simpc_mac 54-89-98-AD-19-A3  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-AD-19-A3" com_port="0" bootmode="0" cx="704.000000" cy="553.000000" edit_left="731" edit_top="607">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="83238DA9-0B69-4e85-A868-6DAE1CA3D89E" name="LSW1" poe="0" model="S3700" settings="" system_mac="4C-1F-CC-DB-2B-50" com_port="2000" bootmode="0" cx="380.000000" cy="350.000000" edit_left="350" edit_top="376">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="22" />
                <interface sztype="Ethernet" interfacename="GE" count="2" />
            </slot>
        </dev>
        <dev id="478FDA80-7B86-47de-9C28-C4A6C68F92B0" name="LSW2" poe="0" model="S3700" settings="" system_mac="4C-1F-CC-F7-25-24" com_port="2001" bootmode="0" cx="704.000000" cy="350.000000" edit_left="781" edit_top="373">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="22" />
                <interface sztype="Ethernet" interfacename="GE" count="2" />
            </slot>
        </dev>
        <dev id="ACCA6D9E-8313-476c-8C68-29B742717893" name="LSW3" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-1C-6F-EB" com_port="2002" bootmode="0" cx="463.000000" cy="150.000000" edit_left="516" edit_top="137">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
        <dev id="ACD66FE9-4C66-4b6e-ABCC-E714AA7E723C" name="LSW4" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-A7-32-D1" com_port="2003" bootmode="0" cx="647.000000" cy="150.000000" edit_left="654" edit_top="134">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="A51DDDDF-B454-4be8-87C4-FDBEFC28939B" destDeviceID="83238DA9-0B69-4e85-A868-6DAE1CA3D89E">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="346.965851" srcBoundRect_Y="539.492432" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="1" tarBoundRect_X="392.034149" tarBoundRect_Y="417.507538" tarOffset_X="-85.000000" tarOffset_Y="-1.000000" />
        </line>
        <line srcDeviceID="5BE3F837-9383-4154-8548-82499F00E916" destDeviceID="83238DA9-0B69-4e85-A868-6DAE1CA3D89E">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="446.672272" srcBoundRect_Y="538.069397" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="1" tarBoundRectIsMoved="1" tarBoundRect_X="417.327728" tarBoundRect_Y="418.930603" tarOffset_X="9.000000" tarOffset_Y="-1.000000" />
        </line>
        <line srcDeviceID="AC4714D7-D1C0-4058-8109-31FAEFDB2A2C" destDeviceID="478FDA80-7B86-47de-9C28-C4A6C68F92B0">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="731.000000" srcBoundRect_Y="536.816223" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="1" tarBoundRect_X="731.000000" tarBoundRect_Y="420.183777" tarOffset_X="9.000000" tarOffset_Y="-2.000000" />
        </line>
        <line srcDeviceID="83238DA9-0B69-4e85-A868-6DAE1CA3D89E" destDeviceID="ACCA6D9E-8313-476c-8C68-29B742717893">
            <interfacePair lineName="Copper" srcIndex="2" srcBoundRectIsMoved="1" srcBoundRect_X="423.552490" srcBoundRect_Y="337.114502" srcOffset_X="-91.000000" srcOffset_Y="-9.000000" tarIndex="0" tarBoundRectIsMoved="1" tarBoundRect_X="473.447510" tarBoundRect_Y="216.885498" tarOffset_X="-61.000000" tarOffset_Y="-5.000000" />
        </line>
        <line srcDeviceID="478FDA80-7B86-47de-9C28-C4A6C68F92B0" destDeviceID="ACCA6D9E-8313-476c-8C68-29B742717893">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="1" srcBoundRect_X="697.768860" srcBoundRect_Y="349.422302" srcOffset_X="-75.000000" srcOffset_Y="11.000000" tarIndex="1" tarBoundRectIsMoved="1" tarBoundRect_X="523.231140" tarBoundRect_Y="204.577698" tarOffset_X="11.000000" tarOffset_Y="-6.000000" />
        </line>
        <line srcDeviceID="83238DA9-0B69-4e85-A868-6DAE1CA3D89E" destDeviceID="ACD66FE9-4C66-4b6e-ABCC-E714AA7E723C">
            <interfacePair lineName="Copper" srcIndex="3" srcBoundRectIsMoved="0" srcBoundRect_X="441.562531" srcBoundRect_Y="351.110443" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="1" tarBoundRect_X="639.437439" tarBoundRect_Y="202.889542" tarOffset_X="-28.000000" tarOffset_Y="15.000000" />
        </line>
        <line srcDeviceID="478FDA80-7B86-47de-9C28-C4A6C68F92B0" destDeviceID="ACD66FE9-4C66-4b6e-ABCC-E714AA7E723C">
            <interfacePair lineName="Copper" srcIndex="2" srcBoundRectIsMoved="1" srcBoundRect_X="719.163940" srcBoundRect_Y="335.469940" srcOffset_X="31.000000" srcOffset_Y="-24.000000" tarIndex="1" tarBoundRectIsMoved="0" tarBoundRect_X="685.836060" tarBoundRect_Y="218.530045" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes>
        <shape type="1" filloption="1" color="8454143" upleftcorner="275,535" width="237" height="109" startpt="0,0" endpt="0,0" borderStyle="0" borderWidth="1" />
        <shape type="1" filloption="1" color="8454016" upleftcorner="671,537" width="124" height="111" startpt="0,0" endpt="0,0" borderStyle="0" borderWidth="1" />
    </shapes>
    <txttips>
        <txttip left="366" top="649" right="415" bottom="666" content="vlan 2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="708" top="652" right="757" bottom="669" content="vlan 3" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="303" top="155" right="450" bottom="187" content="vlanif2 192.168.2.3&#x0D;&#x0A;vlanif3 192.168.3.3" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="718" top="157" right="865" bottom="189" content="vlanif2 192.168.2.4&#x0D;&#x0A;vlanif3 192.168.3.4" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="474" top="83" right="674" bottom="115" content="vlanif2 共享 192.168.2.254&#x0D;&#x0A;vlanif3 共享 192.168.3.254" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="935" top="249" right="1214" bottom="388" content="MSTP&#x0D;&#x0A;&#x0D;&#x0A;区域名称：CAMPUS（意思是“校园”）&#x0D;&#x0A;&#x0D;&#x0A;实例1：vlan2 LSW3作根桥&#x0D;&#x0A;实例2：vlan3 LSW4作根桥&#x0D;&#x0A;&#x0D;&#x0A;根桥的优先级数值要比其他交换机 小" fontname="Consolas" fontstyle="0" editsize="110" txtcolor="-16777216" txtbkcolor="-32640" charset="1" />
    </txttips>
</topo>
